Bae146-300 QT

Note: this checklist is based on real world 146 operating

procedures, and does not necessarily reflect functionality

of this 146 model or panel.

COCKPIT PREP | BEFORE START-UP
AFTER START-UP | READY FOR TAXI
BEFORE TAKEOFF | AFTER TAKEOFF
DESCENT | APPROACH
FINAL APPROACH | AFTER LANDING
PARKING |

To... | Press...
Display/hide GPS | SHIFT+2
Display/hide RADIO | SHIFT+3
Display/hide compass | SHIFT+4

____________________________________
Cockpit Preparation
[ ] Fasten Seatbelt Signs: ON
[ ] Pressurization: SET
[ ] Fuel Panel and QTY: SET AND CHECKED
[ ] Flow Meters: ZEROED
[ ] Gear Lights: 3 GREEN
[ ] Flight Data Recorder: SET
[ ] Rudder/All. Trim: 0/0
[ ] GNS Setup: COMPLETED
[ ] Speedbugs: SET
[ ] T/O Data and TMS: SET AND OFF
[ ] T/O Trim: SET
TOP

____________________________________
Before Startup
[ ] Parking Brake: SET
[ ] Brake Fans: OFF
[ ] Hydraulics: ALL OFF
[ ] Fuel Pumps: ALL ON
[ ] Pack 2, APU Air: OFF, OFF
[ ] MWS Test Button: PUSHED
[ ] Windows: SECURED
[ ] Door Lights: Out
[ ] Cabin Secure for Taxi: RECEIVED
[ ] Beacon/Wing Lights: ON/ON
[ ] Start PWR/MST/SEL: NORM/ON/ENG

TOP

____________________________________
After Startup
[ ] Start PWR/MST/SEL: NORM/OFF/OFF
[ ] Engine Anti-Ice: AS REQUIRED
[ ] Generator #1 and #4: CHECKED, BOTH ON
[ ] Hydraulics: ALL ON, CHECKED
[ ] Brake Fans: AUTO
[ ] Pack 2, APU Air: ON, ON
[ ] Heaters: ALL ON
[ ] Ice Detect: ON
[ ] GNS and TMS: ENTERED AND ON

TOP

____________________________________
Ready for Taxi
[ ] Turn. Instr./ Yaw Dampers.: CHECKED, OPPOS
[ ] Flaps: SET
[ ] Airbrake/ Spoilers: CHECKED, In Detent
[ ] Takeoff Trim: Re-Checked
[ ] Config Warning: CHECKED
[ ] Brakes: CHECKED GREEN, YELLOW
[ ] Stobes: ON
[ ] Takeoff Briefing: COMPLETE
[ ] NAV-Settings: AS CLEARED

TOP

____________________________________
Before Takeoff
[ ] Cabin Secure for T/O: RECEIVED
[ ] Transponder: ON
[ ] WX-Radar: AS REQUIRED
[ ] Flight Controls: CHECKED
[ ] Ignition: AS REQUIRED
[ ] MWS: CHECKED
[ ] TMS: TAKEOFF
[ ] RWY-Heading: CHECKED
[ ] Lights: TAKEOFF

TOP

____________________________________
After Takeoff
[ ] Gear: UP, NO LIGHTS
[ ] Flaps: ZERO
[ ] Engine Air: ALL ON
[ ] APU Air: OFF
[ ] Packs: BOTH ON
[ ] APU: STOPPED
[ ] AC PUMP: OFF
[ ] TMS: AS REQUIRED
[ ] Cabin Pressure: CHECKED, NORMAL
[ ] Altimeters: X-CHECKED

TOP

____________________________________
Descent
[ ] Approach Briefing: COMPLETED
[ ] Fasten Seatbelt Signs: ON
[ ] Cabin Pressure: SET, CHECKED NORMAL
[ ] Speed Bugs: SET
[ ] Landing Data: SET, X-CHECKED

TOP

____________________________________
Approach
[ ] Altimeters: SET, X-CHECKED
[ ] Fuel Panel: SET
[ ] No Smoking Sign: ON
[ ] APU: STARTED, CHECKED
[ ] Pack 1: OFF
[ ] APU Air: AS REQUIRED
[ ] Engine Air: AS REQUIRED

TOP

____________________________________
Final Approach
[ ] Gear: DOWN, 3 GREEN
[ ] Brake Pressure: CHECKED
[ ] Flaps: SET, INDICATING 24
[ ] Cabin Secure for Land: RECEIVED
[ ] Flaps: SET, INDICATING 33
[ ] Lights: LANDING, ON

TOP

____________________________________
After Landing
[ ] Transponder: STANDBY
[ ] Lights: TAXI, ON
[ ] Airbrake/ Spoilers: IN
[ ] WX-Radar: OFF
[ ] TMS: OFF
[ ] Engine Anti-Ice: AS REQUIRED
[ ] Ignition: OFF
[ ] Heaters: ALL OFF
[ ] Ice Detect: OFF
[ ] Strobes: OFF
[ ] Flaps: SET, INDICATING 0
[ ] Generator #1 and #4: BOTH OFF, RESET
[ ] Trims: 4.5/0/D SEL.

TOP

____________________________________
Parking
[ ] Parking Brake: SET, PRESSURE CHECKED
[ ] Collumn: LOCKED
[ ] Hydraulics: ALL OFF
[ ] Thrust Levers: FUEL OFF
[ ] Fuel Pumps: 1/2/3/4 OFF
[ ] Fasten Seatbelts Signs: OFF
[ ] Brake Fans: AS REQUIRED
[ ] Engine Anti-Ice: ALL ON
[ ] Beacon/Wing Lights: OFF/OFF
[ ] MWS Test Button: PULLED

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.